Device 0 (VID=0421 and PID=0154) is a Nokia 5800 XpressMusic.
PTP_ERROR_IO: failed to open session, trying again after resetting USB interface
LIBMTP libusb: Attempt to reset device
libmtp version: 1.1.3

Listing raw device(s)
   Found 1 device(s):
   Nokia: 5800 XpressMusic (0421:0154) @ bus 2, dev 10
Attempting to connect device(s)
USB low-level info:
   Interface has a kernel driver attached.
   bcdUSB: 512
   bDeviceClass: 2
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0421
   idProduct: 0154
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 2
      Device number: 10
      Device entry info:
         Vendor: Nokia
         Vendor id: 0x0421
         Product: 5800 XpressMusic
         Vendor id: 0x0154
         Device flags: 0x00000001
Configuration 0, interface 0, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: Nokia
   Model: 5800 XpressMusic
   Device version: 01
   Serial number: 357988032559978
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com:1.0;microsoft.com/WMPPD: 11.0;microsoft.com/WMDRMPD: 10.1;vodafone.com/omadrmv2: 1.0
   Detected object size: 64 bits
   Extensions:
        microsoft.com: 1.0
        microsoft.com/WMPPD: 11.0
        microsoft.com/WMDRMPD: 10.1
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9810: Get object references
   9811: Set object references
   9805: Get object property list
   9806: Set object property list
   9807: Get interdependent property description
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9203: Get transferable playlist types
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
Events supported:
   0x400a
   0x4004
   0x4005
   0x4003
Device Properties Supported:
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd404: Unknown property
   0xd303: Unknown property
   0xd102: Device Certificate
   0xd406: Session Initiator Info
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   b903: AAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 41222,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 41222,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 85,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 41222,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b004: Unknown(b004)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 1, 85, 41222,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 41222,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 176, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 144, MAX 240, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type ANY 16BIT VALUE form GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911, 1297101377, 1297101889,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 384000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc87: Width UINT32 data type range: MIN 176, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 144, MAX 240, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type ANY 16BIT VALUE form GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 384000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      dc94: Parental Rating STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   ba11: M3U Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 1,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 16000, MAX 1536000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00040001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 8022654976
      FreeSpaceInBytes: 0
      FreeSpaceInObjects: 0
      StorageDescription: Memory card (5800XM_8GB)
      VolumeIdentifier: 272687601
   StorageID: 0x00020001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 90210304
      FreeSpaceInBytes: 0
      FreeSpaceInObjects: 0
      StorageDescription: Phone memory
      VolumeIdentifier: 734637202
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0xffffffff
   Default picture folder: 0xffffffff
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: Nokia 5800 XpressMusic
   Synchronization partner: Nokia 5800 XpressMusic
libmtp supported (playable) filetypes:
   Folder
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   ISO MPEG-1 Audio Layer 3
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   Abstract Playlist file
   RIFF WAVE file
OK.
