~$ mtp-detect

libmtp version: 0.3.3

Listing raw device(s)
 Found 1 device(s):
 1043:1143 @ bus 0, dev 9
Attempting to connect device(s)
USB low-level info:
 Using kernel interface "usbfs"
 bcdUSB: 512
 bDeviceClass: 255
 bDeviceSubClass: 0
 bDeviceProtocol: 0
 idVendor: 1043
 idProduct: 1143
 IN endpoint maxpacket: 512 bytes
 OUT endpoint maxpacket: 512 bytes
 Raw device info:
    Bus location: 0
    Device number: 9
    Device entry info:
       Vendor: (null)
       Vendor id: 0x1043
       Product: (null)
       Vendor id: 0x1143
       Device flags: 0x00000000
Microsoft device descriptor 0xee:
  0000: 1203 4d00 5300 4600 5400 3100 3000 3000    ..M.S.F.T.1.0.0.
  0010: fe00                                       ..
Microsoft device response to control message 1, CMD 0xfe:
  0000: 2800 0000 0001 0400 0100 0000 0000 0000    (...............
  0010: 0001 4d54 5000 0000 0000 0000 0000 0000    ..MTP...........
  0020: 0000 0000 0000 0000                        ........
Microsoft device response to control message 2, CMD 0xfe:
  0000: 2800 0000 0001 0400 0100 0000 0000 0000    (...............
  0010: 0001 4d54 5000 0000 0000 0000 0000 0000    ..MTP...........
  0020: 0000 0000 0000 0000                        ........
Device info:
 Manufacturer: iriver
 Model: iriver T7
 Device version: MTP-1.01-N-ENG
 Serial number: A00000600001
 Vendor extension ID: 0x00000006
 Vendor extension description: microsoft.com: 1.0;
microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
 Detected object size: 64 bits
Supported operations:
 1001: get device info
 1002: Open session
 1003: Close session
 1004: Get storage IDs
 1005: Get storage info
 1006: Get number of objects
 1007: Get object handles
 1008: Get object info
 1009: Get object
 100b: Delete object
 100c: Send object info
 100d: Send object
 100f: Format storage
 1010: Reset device
 1014: Get device property description
 1015: Get device property value
 1016: Set device property value
 9801: Get object properties supported
 9802: Get object property description
 9803: Get object property value
 9804: Set object property value
 9810: Get object references
 9811: Set object references
 9101: Get secure time challenge
 9102: Get secure time response
 9103: Set license response
 9104: Get sync list
 9105: Send meter challenge query
 9106: Get meter challenge
 9107: Get meter response
 9108: Clean data store
 9109: Get license state
Events supported:
 0x4004
 0x4005
Device Properties Supported:
 0xd101: Secure Time
 0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
 3000: Undefined Type
    dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
    dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
    dc04: ObjectSize UINT64 data type READ ONLY
    dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
    dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
    dc44: Name STRING data type GET/SET
    dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
 3001: Association/Directory
    dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
    dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
    dc04: ObjectSize UINT64 data type READ ONLY
    dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
    dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
    dc44: Name STRING data type GET/SET
    dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
 3009: MP3
    dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
    dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
    dc04: ObjectSize UINT64 data type READ ONLY
    dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
    dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
    dc44: Name STRING data type GET/SET
    dc46: Artist STRING data type GET/SET
    dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
    dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
    dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
    dc8c: Genre STRING data type GET/SET
    dc96: Composer STRING data type GET/SET
    dc9a: AlbumName STRING data type GET/SET
    de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
    de94: NumberOfChannels UINT16 data type enumeration: 2,  READ ONLY
    de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 READ ONLY
 b901: WMA
    dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
    dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
    dc04: ObjectSize UINT64 data type READ ONLY
    dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
    dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
    dc44: Name STRING data type GET/SET
    dc46: Artist STRING data type GET/SET
    dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
    dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
    dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
    dc8c: Genre STRING data type GET/SET
    dc96: Composer STRING data type GET/SET
    dc9a: AlbumName STRING data type GET/SET
    de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
    de94: NumberOfChannels UINT16 data type enumeration: 2,  READ ONLY
    de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 READ ONLY
 ba03: Abstract Audio Album
    dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
    dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
    dc04: ObjectSize UINT64 data type READ ONLY
    dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
    dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
    dc44: Name STRING data type GET/SET
    dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
    dc81: RepresentativeSampleFormat UINT16 data type enumeration:  READ ONLY
    dc8c: Genre STRING data type GET/SET
 ba05: Abstract Audio Video Playlist
    dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
    dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
    dc04: ObjectSize UINT64 data type READ ONLY
    dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
    dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
    dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
    dc44: Name STRING data type GET/SET
    dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
 StorageID: 0x00010001
    StorageType: 0x0004 removable RAM storage
    FilesystemType: 0x0002 generic hierarchical
    AccessCapability: 0x0000 read/write
    MaxCapacity: 4059193344
    FreeSpaceInBytes: 4059160576
    FreeSpaceInObjects: 4294967295
    StorageDescription: iriver T7 files
    VolumeIdentifier: (null)
Special directories:
 Default music folder: 0x00000000
 Default playlist folder: 0x00000000
 Default picture folder: 0x00000000
 Default video folder: 0x00000000
 Default organizer folder: 0x00000000
 Default zencast folder: 0x00000000
 Default album folder: 0x00000000
 Default text folder: 0x00000000
MTP-specific device properties:
 Friendly name: (NULL)
 Synchronization partner: (NULL)
libmtp supported (playable) filetypes:
 ISO MPEG-1 Audio Layer 3
 Microsoft Windows Media Audio

Secure Time:
<DRMCLOCK type="status"><VALUE>#20080114
19:26:48Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">nrDQMNYHb0qoz1fqYUDqxmFA6sY=</UNIQUEID><PUBLICKEY
private="1">WbWEVwzD/6k56XKst4OnRTXFJSFurpcN/nEqZeM8/1nMhaqcqrUEQw==</PUBLICKEY><KEYDATA>yZBMmoENcUJrZlqoKjB3RqWbZBk=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>WbWEVwzD/6k56XKst4OnRTXFJSENGS5l+4hHr9gLDu1ThP1y59iwSQ==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>AZDXn3sieh4rYaQNQl/MdIAKcL0=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.111.31</SECURITYVERSION><CERTIFICATE
private="1">WbWEVwzD/6k56XKst4OnRTXFJSFurpcN/nEqZeM8/1nMhaqcqrUEQwIEbx9ZtYRXDMP/qTnpcqy3g6dFNcUlIf4NogOPQJYt/s2w7iE5BAM/r9Iq</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>T7</NAME><MANUFACTURER>iriver</MANUFACTURER><MAKE>iriver</MAKE><DISTRIBUTOR>iriver</DISTRIBUTOR><MODEL>T7</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><HARDWARE_VER_MAJOR>1.0</HARDWARE_VER_MAJOR><HARDWARE_VER_MINOR>1.0</HARDWARE_VER_MINOR><FIRMWARE_VER_MAJOR>1.0</FIRMWARE_VER_MAJOR><FIRMWARE_VER_MINOR>1.0</FIRMWARE_VER_MINOR><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>0</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>0</ENCRYPTION><SYMMETRIC_OPT>0</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>6656</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>3BpF6JtA7FbR1nASAkawbHYRtEWT5o8TrP7a2L6Bvxb7/P0+i5NLLA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>WRTND1A2JBpLj8Qsi40ZqMRWx4h/7FCW2OCTmtILKq2DJfeA99WGVg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2691</AUTH_ID><PUBLICKEY>WmzVzzbfShRhYsmIVMx/NHFUoxx4e0Mw84ZZX/Jkb5TDaeO2+Y3whA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>GU1KjL5g1ZWk23mePnHrT1lJSWscoAt36qwgV2jL+BX5R/uUTr3ADg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>97tzJe/maHwwV07tt0FoMe84Hn9adZfKZ7PJ9j3dWh11FiAzG8jxJA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
OK.
