Error: Unable to open ~/.mtpz-data for reading.
libmtp version: 1.1.5

Listing raw device(s)
   Found 1 device(s):
   Philips: GoGear Vibe/02 (0471:20e5) @ bus 2, dev 5
Attempting to connect device(s)
USB low-level info:
   Interface has a kernel driver attached.
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0471
   idProduct: 20e5
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 2
      Device number: 5
      Device entry info:
         Vendor: Philips
         Vendor id: 0x0471
         Product: GoGear Vibe/02
         Vendor id: 0x20e5
         Device flags: 0x00000002
Device info:
   Manufacturer: Philips
   Model: Philips GoGear ViBE
   Device version: 2.02
   Serial number: 400400009D0CDC190002DCE4AF289C19
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/DeviceServices: 1.0; microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0; microsoft.com/WMPPD: 11.0; ; audible.com: 1.0
   Detected object size: 64 bits
   Extensions:
        microsoft.com/DeviceServices: 1.0
        microsoft.com: 1.0
        microsoft.com/WMDRMPD: 10.1
        microsoft.com/WMPPD: 10.0
        microsoft.com/WMPPD: 11.0
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   100f: Format storage
   9810: Get object references
   9811: Set object references
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9203: Get transferable playlist types
   97f1: Unknown (97f1)
   97f2: Unknown (97f2)
   97f3: Unknown (97f3)
   97f4: Unknown (97f4)
   97f5: Unknown (97f5)
   97fa: Unknown (97fa)
   1010: Reset device
   1012: Set object protection
   9807: Get interdependent property description
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd402: Friendly Device Name
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd405: Device Icon
   0x5001: Battery Level
   0xd303: Unknown property
   0xd100: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 4300000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 80, 85,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 2304000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 17,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 256000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 352, 353,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   b906: FLAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 352, 353,  GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30050, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 5000, MAX 768010, STEP 1 READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   ba11: M3U Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   b908: Unknown(b908)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   b904: Audible.com Codec
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      da00: Unknown property UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  READ ONLY
      da02: Unknown property UINT32 data type ANY 32BIT VALUE form GET/SET
      da01: Unknown property STRING data type READ ONLY
      da03: Unknown property UINT16 data type enumeration: 0, 1,  GET/SET
      da04: Unknown property UINT128 data type READ ONLY
   b301: Unknown(b301)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      da00: Unknown property UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  READ ONLY
      da02: Unknown property UINT32 data type ANY 32BIT VALUE form GET/SET
      da01: Unknown property STRING data type READ ONLY
      da03: Unknown property UINT16 data type enumeration: 0, 1,  GET/SET
      da04: Unknown property UINT128 data type READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 3757039616
      FreeSpaceInBytes: 3664297984
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal Storage
      VolumeIdentifier: 400400009D0CDC190002DCE4AF289C19
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0x000000a9
   Default picture folder: 0x0000006c
   Default video folder: 0x000000a2
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: Philips GoGear ViBE
   Synchronization partner: Philips GoGear ViBE
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   RIFF WAVE file
   Microsoft Windows Media Audio
   Free Lossless Audio Codec (FLAC)
   Microsoft Advanced Systems Format
   Folder
   Abstract Playlist file
   JPEG file
   GIF bitmap file
   BMP bitmap file
   Abstract Album file
   Audible.com Audio Codec
OK.
