libmtp version: 1.0.3

Listing raw device(s)
Device 0 (VID=0fce and PID=013a) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
   Found 1 device(s):
   0fce:013a @ bus 2, dev 7
Attempting to connect device(s)
broken! 827af030 not found
broken! 88b98200 not found
broken! a9c00006 not found
broken! adff96d7 not found
broken! b6780000 not found
broken! dc020082 not found
broken! dc440082 not found
broken! e57cce8e not found
broken! f0000000 not found
broken! ffdc0700 not found
broken! 0 not found
broken! 0 not found
broken! 0 not found
broken! 0 not found
broken! 82798800 not found
broken! 82b6f000 not found
broken! 8d0008dc not found
broken! ac20ffff not found
broken! b03835df not found
broken! dc010082 not found
broken! dc4e0082 not found
broken! f0b98200 not found
broken! ffdc0700 not found
broken! 1 not found
broken! 200065 not found
broken! 310030 not found
broken! 3210ff not found
broken! 340070 not found
broken! 620075 not found
broken! 650068 not found
broken! 660064 not found
broken! 66006f not found
broken! 7a10ffff not found
broken! 7a10ffff not found
broken! dc410082 not found
broken! dc410082 not found
broken! e8000200 not found
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0fce
   idProduct: 013a
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 2
      Device number: 7
      Device entry info:
         Vendor: (null)
         Vendor id: 0x0fce
         Product: (null)
         Vendor id: 0x013a
         Device flags: 0x00000000
Configuration 0, interface 0, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: SonyEricsson
   Model: U8i
   Device version: 01
   Serial number: 012305003580353
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com:1.0;microsoft.com/WMPPD: 11.0;vodafone.com/omadrmv2: 1.0
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9810: Get object references
   9811: Set object references
   9805: Get object property list
   9806: Set object property list
   9807: Get interdependent property description
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9203: Get transferable playlist types
Events supported:
   0x400a
   0x4004
   0x4005
   0x4003
Device Properties Supported:
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd404: Unknown property
   0xd406: Session Initiator Info
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   b903: AAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b004: Unknown(b004)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 176, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 144, MAX 240, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type ANY 16BIT VALUE form GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911, 1297101377, 1297101889,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 384000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc87: Width UINT32 data type range: MIN 176, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 144, MAX 240, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type ANY 16BIT VALUE form GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 384000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      dc94: Parental Rating STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   ba11: M3U Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: Date Added STRING data type DATETIME FORM READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00040001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 7927611392
      FreeSpaceInBytes: 6922014720
      FreeSpaceInObjects: 3306
      StorageDescription: Memory card (PHONE CARD)
      VolumeIdentifier: 1138963242
   StorageID: 0x00020001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 75633664
      FreeSpaceInBytes: 38864384
      FreeSpaceInObjects: 18
      StorageDescription: Phone memory (NO NAME)
      VolumeIdentifier: 1270601559
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0x00818010
   Default picture folder: 0xffffffff
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: SonyEricsson U8i
   Synchronization partner: {00000000-0000-0000-0000-000000000000}
libmtp supported (playable) filetypes:
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   ISO MPEG-1 Audio Layer 3
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   Abstract Playlist file
   RIFF WAVE file
Segmentation fault

