libmtp version: 0.2.6.1

Attempting to connect device(s)
Device 1 (VID=1e53 and PID=0006) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp
development team
PTP: Opening session
Detect: Successfully connected 1 devices
Error 2: PTP Layer error 02fe: get_all_metadata_fast(): could not get
proplist of all objects.
Error 2: (Look this up in ptp.h for an explanation.)
USB low-level info:
   Using kernel interface &quot;usbfs&quot;
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 1e53
   idProduct: 0006
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000000
Microsoft device descriptor 0xee:
        0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
        0010: 0100                                      ..
Microsoft device response to control message 1, CMD 0x01:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000                       ........
Microsoft device response to control message 2, CMD 0x01:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000                       ........
Device info:
   Manufacturer: 02 media
   Model: ZoltarTV
   Device version: 1.0
   Serial number: 0000000000000000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0;
microsoft.com/WMPPD: 10.0
   Detected object size: 64 bits
Supported operations:
   1002: Open session
   1003: Close session
   1001: get device info
   1014: Get device property description
   1004: Get storage IDs
   1005: Get storage info
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100c: Send object info
   100d: Send object
   1015: Get device property value
   100b: Delete object
   9802: Get object property description
   9803: Get object property value
   9801: Get object properties supported
   9805: Get object property list
   9804: Set object property value
Events supported:
   0x4001
   0x4002
   0x4003
   0x4006
   0x4007
Device Properties Supported:
   0xd405: Device Icon
   0xd407: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3001: Association/Directory
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3009: MP3
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3008: MS Wave
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   b901: WMA
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   b902: OGG
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3007: AIFF
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   b903: AAC
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   300c: ASF
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3801: JPEG
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3804: BMP
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   300a: MS AVI
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3000: Undefined Type
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3800: Defined Type
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   b900: Undefined Audio
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   b980: Undefined Video
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   300b: MPEG
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   380b: PNG
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   3807: GIF
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   380d: TIFF
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   ba11: M3U Playlist
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   b984: 3GP
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
   b982: MP4
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
Storage Devices:
   StorageID: 0x10000001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 1498410237952
      FreeSpaceInBytes: 1489321717760
      FreeSpaceInObjects: 4294967295
      StorageDescription: Local HDD
      VolumeIdentifier: 0123456789
Special directories:
   Default music folder: 0x00000002
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: (NULL)
   Synchronization partner: (NULL)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   RIFF WAVE file
   Microsoft Windows Media Audio
   Ogg container format
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Microsoft Advanced Systems Format
   JPEG file
   BMP bitmap file
   Audio Video Interleave
   Undefined audio file
   Undefined video file
   MPEG video stream
   Portable Network Graphics
   GIF bitmap file
   TIFF bitmap file
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
Unable to acquire device certificate, perhaps this device does not support this
WMPInfo.xml Does not exist on this device
PTP: Closing session
OK.
