hal# mtp-detect 
libmtp version: 0.2.1

Attempting to connect device(s)
Potential MTP Device with VendorID:0fce and ProductID:0076 responded to control message 2 with a response that was too short. Problems may arrise but continuing
Device 1 (VID=0fce and PID=0076) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0fce
   idProduct: 0076
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000000
Microsoft device descriptor 0xee:
        0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
        0010: 0800 0000 0000 0000 0000 0000 0000 0000   ................
        0020: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0030: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0040: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0050: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0060: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0070: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0080: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0090: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0100: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0110: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0120: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0130: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0140: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0150: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0160: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0170: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0180: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0190: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0200: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0210: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0220: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0230: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0240: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0250: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0260: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0270: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0280: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0290: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0300: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0310: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0320: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0330: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0340: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0350: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0360: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0370: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0380: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0390: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
Microsoft device response to control message 1, CMD 0x08:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0030: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0040: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0050: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0060: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0070: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0080: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0090: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0100: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0110: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0120: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0130: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0140: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0150: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0160: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0170: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0180: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0190: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0200: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0210: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0220: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0230: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0240: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0250: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0260: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0270: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0280: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0290: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0300: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0310: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0320: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0330: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0340: 0f0f 0f0f 0f0f 0010 1010 1010 1010 1010   ................
        0350: 1010 1010 1010 1000 6d63 6f75 6e74 3a20   ........mcount: 
        0360: 5072 6f66 696c 696e 6720 6f66 2073 6574   Profiling of set
        0370: 7b75 2c67 7d69 6420 6269 6e61 7269 6573   {u,g}id binaries
        0380: 2069 7320 6e6f 7420 616c 6c6f 7765 6400    is not allowed.
        0390: 5f6d 636c 6561 6e75 703a 2069 6e74 6572   _mcleanup: inter
        03a0: 6e61 6c20 6275 6666 6572 206f 7665 7266   nal buffer overf
        03b0: 6c6f 772c 2050 524f 4644 4952 2074 6f6f   low, PROFDIR too
        03c0: 206c 6f6e 6700 5f6d 636c 6561 6e75 703a    long._mcleanup:
        03d0: 2074 6f73 206f 7665 7266 6c6f 770a 0050    tos overflow..P
        03e0: 524f 4644 4952 0067 6d2f 7573 722f 706b   ROFDIR.gm/usr/pk
        03f0: 6773 7263 2f77 6970 2f6c 6962 6d74 7000   gsrc/wip/libmtp.
Potential MTP Device with VendorID:0fce and ProductID:0076 responded to control message 2 with a response that was too short. Problems may arrise but continuing
Device info:
   Manufacturer: Sony Ericsson
   Model: Sony Ericsson Phone
   Device version: 1.00
   Serial number: 00000000000000000358875011380618
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 11.0; microsoft.com/WMPPD: 10.0; vodafone.com/omadrmv2: 1.0;
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
Events supported:
   0x4004
   0x4005
   0x400a
Device Properties Supported:
   0x5002: Functional Mode
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
   0xd404: Unknown property
   0xd405: Device Icon
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   b984: 3GP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc47: DateAuthored STRING data type GET/SET
Unknown OPFF type 3
      dc99: OriginalReleaseDate STRING data type GET/SET
Unknown OPFF type 3
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc06: AssociationDesc UINT32 data type ANY 32BIT VALUE form GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3004: Text
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3005: HTML
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc47: DateAuthored STRING data type GET/SET
Unknown OPFF type 3
      dc99: OriginalReleaseDate STRING data type GET/SET
Unknown OPFF type 3
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc47: DateAuthored STRING data type GET/SET
Unknown OPFF type 3
      dc99: OriginalReleaseDate STRING data type GET/SET
Unknown OPFF type 3
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc47: DateAuthored STRING data type GET/SET
Unknown OPFF type 3
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3804: BMP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3807: GIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   380b: PNG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   380f: JP2
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   3810: JPX
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc47: DateAuthored STRING data type GET/SET
Unknown OPFF type 3
      dc99: OriginalReleaseDate STRING data type GET/SET
Unknown OPFF type 3
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   b981: WMV
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc47: DateAuthored STRING data type GET/SET
Unknown OPFF type 3
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911,  READ ONLY
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc47: DateAuthored STRING data type GET/SET
Unknown OPFF type 3
      dc99: OriginalReleaseDate STRING data type GET/SET
Unknown OPFF type 3
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
   ba11: M3U Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type READ ONLY
Unknown OPFF type 3
      dc09: DateModified STRING data type READ ONLY
Unknown OPFF type 3
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type ANY 16BIT VALUE form GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      db02: unknown(db02) array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 66351104
      FreeSpaceInBytes: 24440832
      FreeSpaceInObjects: 0
      StorageDescription: Phone Memory
      VolumeIdentifier: 
   StorageID: 0x00020001
      StorageType: 0x0004
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 957020160
      FreeSpaceInBytes: 683114496
      FreeSpaceInObjects: 0
      StorageDescription: Memory Stick (TM)
      VolumeIdentifier: 
Special directories:
   Default music folder: 0x00000056
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x0000002e
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: W910i
   Synchronization partner: Computer
libmtp supported (playable) filetypes:
   Text file
   HTML file
   RIFF WAVE file
   ISO MPEG-1 Audio Layer 3
   Microsoft Advanced Systems Format
   JPEG file
   BMP bitmap file
   GIF bitmap file
   Portable Network Graphics
   JP2 file
   JPX file
   Microsoft Windows Media Audio
   Microsoft Windows Media Video
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
Unable to acquire device certificate, perhaps this device does not support this
Error 2: PTP Layer error 02fe: get_device_unicode_property(): failed to get unicode property.
Error 2: (Look this up in ptp.h for an explanation.)
^C
