libmtp version: 0.1.5

Attempting to connect device(s)
Clearing stall on IN endpoint
Clearing stall on OUT endpoint
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0e79
   idProduct: 1207
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000002
Device info:
   Manufacturer: ARCHOS
   Model: GminiXS100
   Device version: 2.2.02    
   Serial number: FLKMAUF5T26D
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.0; microsoft.com/WMPPD: 10.0;
Supported operations:
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   1001: get device info
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   100f: Format storage
   1010: Reset device
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100c: Send object info
   100d: Send object
   100b: Delete object
   1019: Move object
   101a: Copy object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9807: Get interdependent property description
   9808: Send object property list
   9810: Get object references
   9811: Set object references
Events supported:
   0x4001
   0x4004
   0x4005
   0x400a
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0x5001: Battery Level
   0xd401: Synchronization Partner
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT16 data type ANY 16BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 24000, 32000, 44100, 48000, 64000, 88200, 96000,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 32768, MAX 327680, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT16 data type ANY 16BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 44100, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 192000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT16 data type ANY 16BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 64000, MAX 3072000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 1,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 1, MAX 1024, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 1, MAX 1024, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
Storage Devices:
   StorageID: 0x00100001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 4013948928
      FreeSpaceInBytes: 957349888
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal HardDisk
      VolumeIdentifier: 55P060EYB0F         
Special directories:
   Default music folder: 0x00010aea
   Default playlist folder: 0x00013753
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: (NULL)
   Synchronization partner: (NULL)
   Battery level 3 of 3 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070508 22:36:32Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">FLKMAUF5T26D</UNIQUEID><PUBLICKEY private="1">C6T0O4YiV1Syf44QgH6rbWEvQIJnJmcWIh4cDOpRT25WFXx44tK3RA==</PUBLICKEY><KEYDATA>TWfNxwNlkYXcOTQbFLW3Rn9nIAM=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>v+i6rrtZWJNG43nTNc1GyQY+eD6z0XgqBJNGqWkFDYEp4lCaj+wAKA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>VFN0PggxNcYVvLaq2xaV0v4wwm0=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.102.189</SECURITYVERSION><CERTIFICATE private="1">C6T0O4YiV1Syf44QgH6rbWEvQIJnJmcWIh4cDOpRT25WFXx44tK3RAIEZr3RRxksnJvewfLyatdCDaMVprlYPYMo/abttSM8WCb1bloyYI1Rpq97</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>GminiXS100</NAME>
    <MANUFACTURER>Archos</MANUFACTURER>
    <MAKE>GminiXS100</MAKE>
    <DISTRIBUTOR>Archos</DISTRIBUTOR>
    <MODEL>GminiXS100</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>6</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>2</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
            <PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>0</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>5kaA1WqQfBLdeXSUTteJz8br+zQUWhRVzcnpnTtPSMooEZ2T8k0NCw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>TkIj0q4kQAcQJed6fhgjyPHqzBotfz9ttDERew6IsiViZxsyJ5s9Uw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>545</AUTH_ID><PUBLICKEY>9fhV2ah1sQS39/CSjL1zl9UashRlzQqFQfUdi3IHdxG0dP7Ut73VSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>Jq35cUiQ6fyyDy01ltFcRtSSKQ95wmjPs67dvh3zl9Un83XSBjS9Rw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>ZE56AqYNoyP38mdJVHUx7J6kWjGCP6n1KcB+6LwRxcDhdPPL2trRGA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{DEE8BBA0-88E0-48A4-BFC1-925579726803}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.
