Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 4102
   idProduct: 1116
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x0000001c
Device info:
   Manufacturer: iriver
   Model: iriver U10
   Device version: MTP-1.28-N-FRE
   Serial number: 3e855e73000000fc323030353
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9810: Get object references
   9811: Set object references
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
Events supported:
   None.
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
   0xd101: Secure Time
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type READ ONLY
      dc95: MetaGenre UINT16 data type enumeration: 0, 1, 11, 12, 13, 14, 15, 21, 22, 23, 24, 25, 26, 27, 28, 30,  GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 350000, STEP 1 READ ONLY
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type READ ONLY
      dc95: MetaGenre UINT16 data type enumeration: 0, 1, 11, 12, 13, 14, 15, 21, 22, 23, 24, 25, 26, 27, 28, 30,  GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 350000, STEP 1 READ ONLY
   b902: OGG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 1009516544
      FreeSpaceInBytes: 994571924
      FreeSpaceInObjects: 4294967295
      StorageDescription: iriver U10 files
      VolumeIdentifier: odfiofdhaaaaaampcdadadfdadbdadbd
Special directories:
   Default music folder: 0x000b0000
   Default playlist folder: 0x000e0000
   Default picture folder: 0x00060000
   Default video folder: 0x00070000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00080000
MTP-specific device properties:
   Friendly name: iriver U10
   Synchronization partner: WMP 10; Napster; 
   Battery level 4 of 4 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Ogg container format

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070707 12:21:10Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">CgoKCgoKCgoKCgoKCgoKCgoKCgo=</UNIQUEID><PUBLICKEY private="1">GBqHHaqO+pqv/ONmwK163V+99wcvhIGg8ejENGcqxmDRgatTYT5pLg==</PUBLICKEY><KEYDATA>ImdEQacSpOcuyTX8LShcPujn6ZU=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>8+8w53BteDaRuDYpCUnH7VqsGIXOACG0e1xxhphp0uWeZujfLD0HAQ==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>fJJmQt+jz3ss5lIu0d+AHqspSQo=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.102.3</SECURITYVERSION><CERTIFICATE private="1">GBqHHaqO+pqv/ONmwK163V+99wcvhIGg8ejENGcqxmDRgatTYT5pLgIEZgNTl1aNjjIDx38pP578Ybicaf16IAl67726OApjZ1Jz+QU3dxMnZ5hU</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>iRiver H10 Series</NAME><MANUFACTURER>iRiver</MANUFACTURER><MAKE>iRiver</MAKE><DISTRIBUTOR>ReignCom</DISTRIBUTOR><MODEL>H10</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR><HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR><FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR><FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>1</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>1</ENCRYPTION><SYMMETRIC_OPT>1</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>10240</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>8jeq4PyJZUL8NpU2+/tgvUZC9ijn3RdlK3wd04Iws6oXHoA+D6vFfQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>HZ85tGf5VnDwKLGq2S0OlK/oJCKbCx3A2yudzMOv8ERwi6drHW5xOA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>359</AUTH_ID><PUBLICKEY>DpMhgaZkXUFNFIs4KJe7S9MZYwuE1bBic6AV6wAc7Ir0Stfx8U+SKw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>GWscwHnDoSazgB+YOP2D7xrqDifWEFztujqAWwrkM7onynIcfOBBMQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>QndHdJ4ZoSgvokVCOWsqVnvuckGL5cn6Vrua0j4tcGBrjD9PgNd0AA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{D5ED8A01-F396-4F84-A2E1-41D6776B2BBA}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.
