libmtp version: 0.2.6.1

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 05c6
   idProduct: 3196
   IN endpoint maxpacket: 64 bytes
   OUT endpoint maxpacket: 64 bytes
   Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Microsoft device response to control message 2, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device info:
   Manufacturer: Verizon
   Model: Verizon Music Phone
   Device version: 02.06.015L(148000)
   Serial number: 01307E66
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; 
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1007: Get object handles
   1008: Get object info
   9806: Set object property list
   9808: Send object property list
   100d: Send object
   1009: Get object
   100b: Delete object
   9802: Get object property description
   1014: Get device property description
   9801: Get object properties supported
   9803: Get object property value
   9805: Get object property list
   9810: Get object references
   1015: Get device property value
   1016: Set device property value
   9811: Set object references
   d402: Unknown (d402)
   9804: Set object property value
   1006: Get number of objects
   100c: Send object info
   1012: Set object protection
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9109: Get license state
   9201: Report Added/Deleted Items
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0xd402: Friendly Device Name
   0xd401: Synchronization Partner
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 32000, 44100,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 196608, STEP 1000 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353, 354,  READ ONLY
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 32000, 44100,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 196608, STEP 1000 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
   b700: Unknown(b700)
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 32000, 44100,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 196608, STEP 1000 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration:  READ ONLY
   b701: Unknown(b701)
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 32000, 44100,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 196608, STEP 1000 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration:  READ ONLY
   b702: Unknown(b702)
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 32000, 44100,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 196608, STEP 1000 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration:  READ ONLY
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14344,  GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 65536, STEP 1 READ ONLY
      dc8c: Genre STRING data type GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
   3808: JFIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
Storage Devices:
   StorageID: 0x00020001
      StorageType: 0x0004
      FilesystemType: 0x0000
      AccessCapability: 0x0000
      MaxCapacity: 2012872704
      FreeSpaceInBytes: 1994997760
      FreeSpaceInObjects: 4294967295
      StorageDescription: Removable Storage Card
      VolumeIdentifier: SD02G2£15566592
Special directories:
   Default music folder: 0x000000c8
   Default playlist folder: 0x000000cc
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: V CAST Mobile Phone - External Memory
   Synchronization partner: V CAST Sync Partner
libmtp supported (playable) filetypes:
   Microsoft Windows Media Audio
   ISO MPEG-1 Audio Layer 3
   JPEG file
   JFIF file

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">Zn4wAQAAoMz8YAIAAECY+cEEAAA=</UNIQUEID><PUBLICKEY private="1">ddMq9cyNFb6o3NE7zvUvT3g3Ziz8PC/tmo3SPLhXCXdwbQN19IVkgA==</PUBLICKEY><KEYDATA>2YPGBugfcXZVcgiyC+9uz7kqbak=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>2S1c2qOkOXfFw++/n0XEOmXrOzv7hLVpDkv1yV+w+qnPLICdlNr2hg==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>P2r5oiCTLmJkhyNScalQcVbcT1Y=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.107.183</SECURITYVERSION><CERTIFICATE private="1">ddMq9cyNFb6o3NE7zvUvT3g3Ziz8PC/tmo3SPLhXCXdwbQN19IVkgAIEa7d2suJJstcZ/AJEMe7bk9gywN5aPf4sPX4BsbJRhfQM6t4+88wQKBkF</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>NBalboa</NAME>
    <MANUFACTURER>Nokia</MANUFACTURER>
    <MAKE>Balboa</MAKE>
    <DISTRIBUTOR>Verizon Wireless</DISTRIBUTOR>
    <MODEL>MOD 2.0.0</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>1</CLOCK>
        <METERING>0</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>9cmEszzjSU20vZuhB0ZugY+n8i0mIaDJvA7I45sTBkFGjAsGmi8hWQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>kuca9wotaGTG0G2dPvftj3zxuIahMaIrRG5Wj+lgx6CY4DVFYcgMDw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1819</AUTH_ID><PUBLICKEY>zrP7+pFmhx/HuQJtNEHLEL4zawwFuTDrB1E1l2bc47IC3+KIcYXGMg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>EPs+i571OXLamr1dak7GAPEVYIZzYKAj1seQNfF8zvsfNkD6jxtpbg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>xrtjH01GlxXwSXZJxwRFvkNwGS/Rqoe38IuZT4yaAaU4+mGXEnfVew==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
OK.

 	  	 
