libmtp version: 0.2.1

Attempting to connect device(s)
Potential MTP Device with VendorID:22b8 and ProductID:6415 responded to
control message 2 with a response that was too short. Problems may arrise
but continuing
Device 1 (VID=22b8 and PID=6415) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development
team
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 22b8
   idProduct: 6415
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000000
Microsoft device descriptor 0xee:
        0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
        0010: 1c00                                      ..
Microsoft device response to control message 1, CMD 0x1c:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 3030 0000 0000   ..MTP.....00....
        0020: 0000 0000 0000 0000                       ........
Potential MTP Device with VendorID:22b8 and ProductID:6415 responded to
control message 2 with a response that was too short. Problems may arrise
but continuing
Device info:
   Manufacturer: Motorola
   Model: Z6
   Device version: 1.0
   Serial number: 495534ba190810090909090909090909
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1;
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1012: Set object protection
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9103: Set license response
   9109: Get license state
   9104: Get sync list
   9108: Clean data store
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9101: Get secure time challenge
   9102: Get secure time response
   9106: Get meter challenge
   9107: Get meter response
   9105: Send meter challenge query
   9001: Unknown(9001)
   9002: Unknown(9002)
Events supported:
   0x4001
   0x4004
   0x4005
   0x400b
Device Properties Supported:
   0x5011: Date Time
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
   0xd405: Device Icon
   0xd101: Secure Time
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 100 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2, GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 320000, STEP 1000 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 100 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2, GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 320000, STEP 1000 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 100 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2, GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 320000, STEP 1000 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc06: AssociationDesc UINT32 data type ANY 32BIT VALUE form GET/SET
   3800: Defined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00020001
      StorageType: 0x0004
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 1015529472
      FreeSpaceInBytes: 969621504
      FreeSpaceInObjects: 4294967295
      StorageDescription: MOBILE HANDSET
      VolumeIdentifier: 8368833714948858796012801180231
Special directories:
   Default music folder: 0x00000003
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Z6
   Synchronization partner: Longhorn Sync Engine
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio

Secure Time:
<DRMCLOCK type="status"><VALUE>#20080228
06:36:23Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>AG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">SVU0uhkIEAkJCQkJCQkJCQ==</UNIQUEID><PUBLICKEY
private="1">vBZNMF813hLjiTNHakidsssC1ROzq/ZsKaZuYq8Lx+BfTSoWtmRPAA==</PUBLICKEY><KEYDATA>aBcxvmEvrGKMYj39oM8TS1rC2jQ=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>4yDw58JWBJxZbm6mb/hi7D2M5wuC7q+ZPZq2tCJji55UbK0K9K9WEQ==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>9offoJrDJLDbLVosgEOG9+qyGEk=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.105.89</SECURITYVERSION><CERTIFICATE
private="1">vBZNMF813hLjiTNHakidsssC1ROzq/ZsKaZuYq8Lx+BfTSoWtmRPAAIEaVld8BI9om04YtcY4IgxUhX9tBuJJG3L1N6zdUZn2fIHDAHRnlOYc14o</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>3GPP_Handset</NAME>
    <MANUFACTURER>Motorola</MANUFACTURER>
    <MAKE>ZAS_Platform</MAKE>
    <DISTRIBUTOR>Motorola-DC</DISTRIBUTOR>
    <MODEL>LJ-6.1</MODEL>
    <UNIQUEID>000002B55D10</UNIQUEID>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
           
<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>0</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>0</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   
</LIMITS><PUBLICKEY>XnNQqctLaFox9EIXUgTJqz4Wn2+TVTSVljA2KpkHc8rJOmLJu9SUhg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>OV6UDd4l2t4FwQuj8UwgUJZXanPrPQJgwMO0XM1BY5t+4ACL6AUnQw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1213</AUTH_ID><PUBLICKEY>YwNxtTBKGnuG3NMofm4zTndS9A2mFPoFzDSAWNv5RMNwc8yYok11eQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>0peErT6+EQChZUE788n4ExBoPFdUZbCzKeE2FEJOniRg6HuvkfrhcA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>Byrq7t94b/xMrbc1q5z+icY+PgViUS4ok9e+5S9HWDs+SRbTIq7vTw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
PTP: Closing session
OK.
