libmtp version: 0.3.7

Listing raw device(s)
Potential MTP Device with VendorID:054c and ProductID:03fe responded to control message 2 with a response that was too short. Problems may arrise but continuing
Device 0 (VID=054c and PID=03fe) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
   Found 1 device(s):
   054c:03fe @ bus 0, dev 3
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 054c
   idProduct: 03fe
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 3
      Device entry info:
         Vendor: (null)
         Vendor id: 0x054c
         Product: (null)
         Vendor id: 0x03fe
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: 0100                                   	..
Microsoft device response to control message 1, CMD 0x01:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Potential MTP Device with VendorID:054c and ProductID:03fe responded to control message 2 with a response that was too short. Problems may arrise but continuing
Device info:
   Manufacturer: Sony Corporation
   Model: WALKMAN NWZ-S545
   Device version: 1.00
   Serial number: 00000000000000000000000004056580
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0; microsoft.com/WMPPD: 11.0; sony.net/WMFU: 1.0
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   100f: Format storage
   9810: Get object references
   9811: Set object references
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9203: Get transferable playlist types
   97f1: Unknown (97f1)
   97f2: Unknown (97f2)
   97f3: Unknown (97f3)
   97f4: Unknown (97f4)
   97f5: Unknown (97f5)
   1010: Reset device
   1012: Set object protection
   9807: Get interdependent property description
   9401: Unknown (9401)
   9402: Unknown (9402)
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd402: Friendly Device Name
   0xd401: Synchronization Partner
   0x5001: Battery Level
   0xd405: Device Icon
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 4300000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 80, 85,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 2304000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 17,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 352, 353,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
   b903: AAC
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 41222,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 352, 353,  GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 30050, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 5000, MAX 768010, STEP 1 READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   3807: GIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   3804: BMP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   b981: WMV
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 1478576, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 352, 353,  GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 272, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 30050, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 5000, MAX 1048576, STEP 1 READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   b982: MP4
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 80, 85, 41222,  GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 640, STEP 1 GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 30050, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 5000, MAX 1572864, STEP 1 READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 15840837632
      FreeSpaceInBytes: 10046385512
      FreeSpaceInObjects: 4294967295
      StorageDescription: Storage Media
      VolumeIdentifier: 00000000000000000000000004056580
Special directories:
   Default music folder: 0x00000068
   Default playlist folder: 0x000007ee
   Default picture folder: 0x0000006a
   Default video folder: 0x00000067
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: WALKMAN
   Synchronization partner: WALKMAN NWZ-S545
   Battery level 99 of 100 (99%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   RIFF WAVE file
   Microsoft Windows Media Audio
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Microsoft Advanced Systems Format
   JPEG file
   GIF bitmap file
   BMP bitmap file
   Microsoft Windows Media Video
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)

Secure Time:
<DRMCLOCK type="status"><VALUE>#20100108 02:47:10Z#</VALUE><FLAG>DRM_CLK_NEEDS_REFRESH</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">MDAwMDAwMDEwMDAwMUJBMgoKCgo=</UNIQUEID><PUBLICKEY private="1">gxKzDXjcPHS7rvUP+aVS7QOuXgFZvhQjXWCjZlZsnAzx/enL83rFFA==</PUBLICKEY><KEYDATA>q0KXxVdqWVmkiFG2sz6gKuupRuo=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>D64r+XmsOTWEe5HBhUUVK7SwISfHGGc+PBlVkUSqUWxr6f8RfferVw==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>PRB9gUShd3RqpCEWyr7yUcg3BEk=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.113.179</SECURITYVERSION><CERTIFICATE private="1">gxKzDXjcPHS7rvUP+aVS7QOuXgFZvhQjXWCjZlZsnAzx/enL83rFFAIEcbP3bc+R8W3mJO8kgg80FFiA4xFyE0BZMLOx7BysvFUUUTXA5XhbZMgv</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>Walkman</NAME><MANUFACTURER>Sony</MANUFACTURER><MAKE>Sony</MAKE><DISTRIBUTOR>Sony</DISTRIBUTOR><MODEL>Walkman</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>1</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>1</ENCRYPTION><SYMMETRIC_OPT>1</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>10240</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>WkE5YkC7aJ5pzVrmf5J7ej3ZVoUKwEHAtPv4rkYdvKeuqd8pa+PmMQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>ssMPzjU0Vs/pbxuH8fEGoXxowTRHtIqXrGUqD2uB2cULzsBGCF1oFA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>3351</AUTH_ID><PUBLICKEY>dET+Vay0Z2TNJu6Mf5Dg89UMfXcKfmU0H5Q0M0jDgk0Tuux9nYvkdQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>cA+mkQSGjfKw4MspoToGcx/gLV4uRP6aqZ8c6Gdq1iRYsMuxMqUGbA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>3Qi9EhbnqBCwPf5X9XMFSJvLxjDRxOnz0B/PIENKpFrgBj/NQ9mmhQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
OK.
